|  |  |  |
| --- | --- | --- |
| Hyundai Kona Electric | Standard-range Battery / Motor | Long-range Battery / Motor |

|  |  |
| --- | --- |
| **Battery**  |  |
| Type  | Lithium-ion Polymer | Lithium-ion Polymer |
| Capacity (kWh) | 48.4 | 65.4 |

|  |  |
| --- | --- |
| **Electric motor**  |  |
| Type  | Permanent Magnet Synchronous Motor | Permanent Magnet Synchronous Motor |
| Maximum power |  156 PS / 114.6 kW | 218 PS / 160 kW |
| Maximum torque [Nm] | 255 | 255 |
| 0-100 km/h [s] | 8.8 | 7.8 |
| Top speed [km/h] | 162 | 172 |
| Efficiency (kWh/100 km) | 14.6 | 16.6 - 14.7 |
| CO2 combined (g/km) | 0 | 0 |
| All-electric range (WLTP) [km] | 377 | 514 |

|  |  |
| --- | --- |
| **On-board charger** |  |
| Max. capacity (kW) | 10.4 (3-phase) |

|  |  |
| --- | --- |
| **Charging time**  |  |
| Charge time / standard (AC) 10-100% - 7.4 kW | 6 hours | 8 hours |
| Charge time / standard (AC) 10-100% - 11 kW | 4 hours | 5.4 hours |
| Charge time / quick charge (DC) 10-80% - 50 kW(connected to a 50 kW DC fast charger) | 60 minutes | 60 minutes |
| Charge time / quick charge (DC) 10-80% - 100 kW(connected to a 100 kW DC fast charger) | 41 minutes | 41 min |
| Charge time / ICCB charging 10-100% (3.7 kW 1-phase) | 11.6 hours | 15.4 hours |

|  |  |
| --- | --- |
| **Dimensions exterior** |  |
| Overall length [mm]  | 4,355 |
| Overall width [mm]  | 1,825 |
| Overall height [mm]  | 1,575 – 1,580 |
| Wheelbase [mm] | 2,660 |
| Front overhang/ rear overhang [mm] | 860/835 |
| Ground clearance [mm] | 151 |

|  |  |
| --- | --- |
| **Dimensions interior**  |  |
| Head room front/rear [mm] (with sunroof) | 1,015 (974) / 972 (972) |
| Leg room front/rear [mm]  | 1,059/970 |
| Shoulder room front/rear [mm] | 1,435/1,402 |
| Luggage capacity VDA [l] - seats up | 466 |
| Luggage capacity VDA [l] - seats folded | 1,300 |

|  |  |
| --- | --- |
| **Transmission** |  |
| Automatic | Single Speed Reduction Gear |

|  |
| --- |
| Notes |
|  **Technical specifications listed in this document are tentative and may vary depending on region and trim.** |